**Technical parameters for** **JJJ ( made of CCC ) :**

|  |  |
| --- | --- |
| ****Size**** | ****According to customer’s requirements**** |
| ****Standard**** | ****GB , DIN , JIS , BS , ASTM**** |
| ****Material**** | ****Q235 ; Q345**** |
| ****Surface treatment**** | ****Painted with epoxy paint or zinc rich paint**** |
| ****Package**** | ****In bundle or pallet or according to the requirements of customers**** |
| ****Delivery**** | ****Container or Bulk**** |
| ****Shipment Time**** | ****According to the quantity and specification of each order**** |
| ****Production Usage**** | Used in industrial or civil fields |
| ****Product Characteristics**** | ****1 . Fine gloss exterior , anti-corrosive****  ****2 . High strength , satisfactory property of the steel****  ****3 . Anti-seismic , wind resistance , environmental protection****  ****4 . Fire- resistant , clean and health****  ****5 . 50-year-long life expectancy**** |
| ****Remark**** | ****Payment terms : T/T, L/C**** |
| ****Terms of trade**** | ****FOB , CFR , CIF , EXW**** |