**Data of the JJJ ( made of CCC ) :**

|  |  |
| --- | --- |
| **Specification** | |
| Material : | Grade Q235 , equivalent to ASTM A36  Grade Q345 , equivalent to ASTM A572 |
| Section : | Any product shape according to customer's requirements |
| Certification : | ISO quality system , Chinese GB50221 - 2001 |
| Sand Blast : | SA 2.5 Sand blasting |
| Welding Technology : | Single level butt welding , fillet welding by electric arc welding ,  and Gas shielded welding |
| Surface treatment : | Hot dip galvanized , Epoxy zinc rich primer  Standard : ISO1461 ( 1999 ) , JIS H 8641 - 1999 , ASTM A 123 / A 123M-02 |
| Welding Testing | Ultrasonic Testing , X-ray Testing |
| Manufacturing Technology | Drilling , Cutting , Assembling , Welding , Rectification , Testing etc |