**JJJ ( made of CCC ) **TECHNICAL PARAMETERS:****

|  |  |
| --- | --- |
| Main Steel | Main steel structure -- Q345 / Q235 , etc . Secondary steel structure -- Q235 , etc . can be customized according to customer's requirements . |
| Wide span | Single span or multiple spans , the max span clear distance that we had done is 90m ( without middle column ) . |
| Surface | Painted or Hot Dip Galvanized |
| Connection method | welding connection or bolt connection |
| Column and Beam | Welded H section , Hot Rolled Section Steel , grid column , pipe & tube column . |
| Purlin | C - section or Z - section |
| Roof & Wall Panel | EPS / Rock wool / PU Sandwich panel ;  Single Steel Sheet ( prepainted , Galvanized , Galvalume , etc . ) ;  Fiber glass wool ;  Fireproof paper ;  Transparent panel ( light panel ) ;  Trim ;  Screw , Rivet , Glass glue , etc . |
| Window | Plastic steel , Aluminum alloy , etc . |
| Door | Sliding door , Rolling up door , Industrial Lifting door , etc . |
| Other Accessories | Down pipe , Floor decking panel , Out gutter , Ventilator , Bolts , etc . |
| Service | Design , Detailing , Fabrication and Installation ( *Standard : America Standard , Australia Standard , England Standard , China Standard , etc .* *Design and Detailing software :  SAP2000 , Auto CAD , PKPM , RSTAB , PROE , MTS , 3D3S , Tarch , Tekla Structures ( Xsteel ) , etc.* ) |
| Making quotation according to customer's drawing or as per customer's dimension and requirement ;  Offering a free preliminary design drawing ( formal complete design need to be paid [ high-quality , low-cost ] ) . |
| Packing | We possess the unique most professional and best packaging in China presently - FRAMING PACKAGE , which perfectly protects the structural steel members from any impact damage during the transport . Or according to customer's requirement . |
| Load into 40 / 20GP , 40HQ , 40OT or Bulk carrier |