**Specifications of the JJJ ( made of CCC ) :**

|  |  |
| --- | --- |
| **Main steel frame :** | H section steel beam and columns |
| **Secondary frame :** | Galvanized C / Z purlin , steel bracing , tied bar , knee brace , edge cover etc . |
| **Roof & Wall panel :** | Sandwich panel , corrugated steel sheet or skylight panel |
| **Tie Rod :** | Circular Steel Tube |
| **Brace :** | Round Bar |
| **Knee Brace :** | Angle Steel |
| **Roof Gutter :** | Color Steel Sheet or galvanized Steel sheet |
| **Rainspout :** | PVC Pipe |
| **Door :** | Swing door , sliding door or roller door |
| **Windows :** | PVC steel or Aluminum Alloy Window |
| **Connecting :** | Anchor bolt , high-strength bolt , common bolt |
| **Drawing :** | We can make the design and quotation according to your requirement or your drawing |
| **Installation :** | Provide full set of construction drawings and video to direct installation ; Engineer are able to stay at site to direct construction |