**Technical specs for JJJ ( made of CCC ) :**

|  |  |  |
| --- | --- | --- |
| **Specification** | **Structure type** | **Heavy steel structure** |
| **Design standard** | **AISI / ASTM / BS / DIN / GB / JIS** |
| **Length** | **With customer's requirement** |
| **Width** | **Single span , double-span , multi-span** |
| **Height** | **With customer's requirement** |
| **Components** | **Bolt** | **Steel grade 45** |
| **Column** | **Q235B , Q345B welded H section steel** |
| **Beam** | **Q235B , Q345B welded H section steel** |
| **Tube** | **Steel Q235B ,** **Q345B** |
| **High strength bolt** | **Cr 40 , 10.9S , 9.8S , galvanization** |
| **Sleeve** | **Steel Q235B ,** **Q345B , galvanization** |
| **Purlin** | **Q235B C channel or Z channel , galvanization** |
| **Roof & Wall panel** | **Sandwich panels , Corrugated steel sheet , FRP sheet** |