**Product Details for JJJ ( made of CCC ) :**

|  |  |  |
| --- | --- | --- |
| Main frame | | |
| 1 | Main steel structure    ( columns and beams ) | 1 . Steel Q345 ( S355JR ) or Q235 ( S235JR ) H shape  2 . Straight cross-section or Variable cross - section |
| 2 | Sub steel structure | 1 . Material Q235 ( S235JR ) steel  2 . Bolt connections . Anti-rust painted or galvanized .  3 . Bracing :X - type or V - type or other type bracing made from angle , round pipe , etc  4 . Purlins : C or Z type : Size from C120 ~ C320 , Z100 ~ Z200 |
| Maintenance system | | |
| 3 | Roof | Sandwich panel ( PU / EPS / fiberglass / rook wool ) or Colorful steel tile |
| 4 | Wall | Sandwich panel ( PU / EPS / fiberglass / rook wool ) or Colorful steel tile |
|  | Doors | Steel rolling shutter or others |
|  | Windows | Alu. Alloy window , or others |
| Fitting | | |
| 7 | Edge Cover | Steel sheet 0.5mm thickness |
| 8 | Bolts | M24 , M22 , M16 embedded bolts , intensive bolts , galvanized ordinary bolts , high-strength bolts , etc |
| 9 | Others options | Day - lighting panel , Roof ventilator , Down pipe , Galvanized , Crane , sanitary Products , etc |
| 10 | Foundation | Cement and steel foundation bolts |