**JJJ ( made of CCC ) general classification:**

|  |  |  |
| --- | --- | --- |
| ****( 1 ) Simple Steel Construction**** | | |
| Main structure | Single span : L -****shorter than 18m**** , H -lower than 6m | |
| Maintenance system | Roof | Colored sheet with 50mm glass wool |
| Wall | Colored steel sheet |
| Door | Wind resistance rolling door ( within 10m2 ) |
| Window | Very few |
| Suitable market | No snow , wind load below 0.4kn / m2 | |

|  |  |  |
| --- | --- | --- |
| ****( 2 ) Standard Steel** **Construction**** | | |
| Main structure | Single span : L -****shorter than 24m**** , H -lower than8m | |
| Maintenance system | Roof | Colored sheet with 50mm glass wool |
| Wall | Colored steel sheet or 50mm EPS sandwich board |
| Door | Wind resistance rolling door ( within 15m2 ) |
| Window | Alu. Alloy ( can use with skylight ) |
| Suitable market | Snow loading below 0.5kn , wind loading below 0.5kn / m2 | |

|  |  |  |
| --- | --- | --- |
| ****( 3 ) Coastal ( High Wind Speed )Steel** **Construction**** | | |
| Main structure | Single span : L -****shorter than 18m**** , H -lower than 6 m | |
| Maintenance system | Roof | Colored sheet with 50mm glass wool |
| Wall | Colored steel sheet or 50mm EPS sandwich board |
| Door | Wind resistance rolling door ( within 15m2 ) |
| Window | Alu. Alloy ( can use with skylight ) |
| Suitable market | Snow loading below 0.7kn , wind loading below 1.2kn / m2 | |

|  |  |  |
| --- | --- | --- |
| ****( 4 ) Cold Region ( Heavy Snow ) Steel** **Construction**** | | |
| Main structure | Single span : L -****shorter than 18m**** , H -lower than 6 m | |
| Maintenance system | Roof | Colored sheet with 50mm glass wool |
| Wall | Colored steel sheet or 50mm EPS sandwich board |
| Door | PU foamed rolling door |
| Window | Alu. Alloy ( can use with skylight ) |
| Suitable market | snow loads below 3kn , wind load below 1KN / M2 | |

|  |  |  |
| --- | --- | --- |
| ****( 5 ) Steel** **Construction  with Crane ( 5T , 10T , 15T , 20T )**** | | |
| Main structure | Single span : L -****shorter than 20m**** , H -lower than 10 m | |
| Maintenance system | Roof | Colored sheet with 50mm glass wool |
| Wall | Colored steel sheet or 50mm EPS sandwich board |
| Door | Wind resistance rolling door ( within 15m2 ) |
| Window | Alu. Alloy ( can use with skylight ) |
| Suitable market | Snow 0.5kn , wind load below 0.5kn / m2 | |