****The specifications of** JJJ ( made of CCC ) **:****

|  |  |  |  |
| --- | --- | --- | --- |
| Standard : | GB50661 JGJ81 BS4592 ASM  JIS ISO | Size : | depend on your drawing |
| Material : | Q235 Q345  Welded H Beam and Hot Rolled Section Steel | Grade : | Grade B |
| Material : | low carbon steel | Roofing : | single steel sheet , RW , EPS , PU , XPS , PF |
| Wall panel : | single steel sheet , RW , EPS , PU , XPS , PF | Color : | Red , blue , white or customized |
| Life Time : | 10 - 15 years at least | Manufacturing Method : | Cutting , welding , painting , packing |
| Performance : | Durable , widely using , anti - earthquarke , heat preservation , wind - resistance | Application Fields : | Plant , warehouse , office building , aeroshed , high-riser building etc |
| UOM : | SQM | FOB price : | US$15 - 45 per SQM |
| Supply Ability : | 1500t / month | Delivery Time : | 30 - 45 days depend on the case |
| Package Method : | bulk packing , frame packed , pallet packed , also can be negotiable | Customization Service : | Yes |
| Advantages : | 1 , Save your working time because of its quickly assembly .  2 , Saving energy , as it uses insulated panel with heat preservation and insulation function .  3 , Healthy and eco-friendly ;  4 , Sound proof | | |