**JJJ ( made of CCC ) products description :**

|  |  |  |
| --- | --- | --- |
| Dimensions | Length | H beam : 4000 - 15000mm |
| Thickness | web plate : 6 - 32mm  wing plate : 6 - 40mm |
| Height | 200 - 1200mm |
| Color | Depend on customers’ needs |
| Advantages | 1 . Design according to customers’ requirements | |
| 2 . Manufacture under complete quality control system --- ISO9001 | |
| 3 . Installation with instruction of experienced engineers | |
| 4 . Easy to assemble and dismantle | |
| 5 . Eco-friendly material: can be used for several times and recyclable | |
| 6 . Short construction period , long using time | |
| 7 . High strength and stiffness , high weight bearing. | |
| 8 . Sound insulation and heat insulation ; antisepsis and damp proofing ; waterproof and aseismatic | |
| Main components | Main frame | H beam |
| Purlin | C or Z section steel purlin |
| Brace | Anchor , ordinary , high strength bolt |
| Bolt | Sandwich panel or steel plate |
| Roof &wall | PVC or aluminum alloy door |
| Door | Sliding or rolling door |
| Insulation panel | EPS , Rock wool , PU sandwich |
| Material | Q235B Q345B  China standard steel |
| Sheet | 0.5mm or 0.6mm galvanized sheet |