Technical specs of the **JJJ ( made of CCC ) :**

The **JJJ ( made of CCC )** were designed , constructed and installed by us who are professional on designing , processing and installing of steel structure building . You may give us your own drawings to enable us construct as per your request or you might just give us your ideas , we can design the project based on your ideas . Buildings of steel structure are safe , easy to install and disassemble . This steel structure can be used multiple times without special tools .

1 ) size :

MOQ is 1000 square meter , length X width X eave height , roof slope

2 ) type :

single slope , double slope , muti-slope ; single span ,

double-span , Multi-span , single floor , double floors

3 ) base :

Concrete and steel foundation bolts

4 ) column and beam :

material Q345 ( S355JR ) or Q235 ( S235JR ) steel , all bolts connection , straight cross-section or Variable cross-section

5 ) bracing :

X or V or other type bracing made from angle , round pipe etc .

6 ) c or z purlin ,

size from C100 ~ C320 , Z160 ~ Z300

7 ) roof and wall panel :

single colorful corrugated steel sheet 0.326 ~ 0.6mm thick , YX26-205-820 ( 820mm wide )

single colorful corrugated steel sheet 0.326 ~ 0.6mm thick , YX15-225-900 ( 900mm wide )

single colorful corrugated steel sheet 0.326 ~ 0.6mm thick , YX35-125-750 ( 750mm wide )

single colorful corrugated steel sheet 0.376 ~ 0.6mm thick , YX51-380-760 ( 760mm wide )

single colorful corrugated steel sheet 0.376 ~ 0.6mm thick , YX51-470 ( 470mm wide )

sandwich panel with EPS , rock wool , glass wool , PU etc insulation thickness around 50mm ~ 150mm , width 950mm or 960mm !

8 ) accessories :

Semi - transparent skylight belts , Ventilators , down pipe , out gutter etc

9 ) surface :

Paint or hot dip galvanized

10 ) packing :

main steel frame without packing load in 40'OT , roof and wall panel load in 40' HQ