**JJJ ( made of CCC ) main components :**

|  |  |
| --- | --- |
| ****SIZE(m)**** | LENGTH \* WIDTH \* EAVE HEIGHT |
| ****TYPE**** | SINGLE SPAN , DOUBLE SPAN , MULTI - SPAN |
| ONE FLOOR , TWO FLOORS , THREE FLOORS |
| ****BUILDING FOUNDATION**** | STEEL FOUNDATION WITH ANCHOR BOLTS |
| ****COLUMN & BEAM**** | MATERIA L :Q235B & Q345B |
| ****BRACING**** | X or V TYPE BRACING MADE BY ANGEL STEEL , ROUND Bar etc |
| ****Wall & Roof C or Z PURLINE**** | SIZE :C120 ~ C320mm ; Z100 ~ Z300mm |
| ****WALL & ROOF PANEL**** | SINGLE CORRUGATED STEEL SHEET |
| SANDWICH PANEL INSULATION WITH EPS , PU , ROCK WOOL etc |
| ****WINDOW & DOOR**** | PVC or ALUMINIUM ALLOY WINDOW |
| ELECTRIC ROOL - UP DOOR |
| SLIDING DOOR BY SANDWICH PANEL OR SINGLE CORRUGATED STEEL SHEET |
| ****SURFACE TREATMENT**** | HOT GALVANIZED COATING COLD GALVANIZING |
| Spray - Painting , Any color , or according to your request |
| ****ACCESSIORES**** | SEMI - TRANSPARENT SKYLIGHT BELTS |
| VENTILATORS ; DOWN PIPE ; GUTTER |
| STANDARD BOLTS |