**Products description for the JJJ ( made of CCC ) :**

|  |  |
| --- | --- |
| Main Steel | |
| Steel Beam Column | Q235B , Q345B |
| Secondary Steel | |
| Tie Bar | Q235B |
| Purlin | C and Z purlin |
| Bracing | Q235B |
| Accessories | |
| Surface | Painted or Hot Dip Galvanized |
| Door | Rolling Up Door or Sliding Door |
| Window | PVC or Aluminum Alloy |
| Roof and Wall Panels | Corrugated Steel Sheet , EPS Sandwich Panel , Rock Wool Sandwich  Panel , PU Sandwich Panel |
| Others | |
| Service | Design , Fabrication and Installation |
| We can offer quotations according to customers’ drawings and requirements , free design drawings and detailed installation drawings . |
| Design software :  Auto CAD , PKPM , MTS , 3D3S , TArch , Tekla Structures ( X steel ) V12.0 , etc |
| Packing | main steel frame with 40 OT  roof and panel load in 40 HQ  Or According To Customer Requirement |