**Specifications for the JJJ ( made of CCC ) :**

|  |  |
| --- | --- |
| Items | Specification |
| Length | Single slope , double slope , muti slope |
| Width | Single span , double-span , Multi-span |
| Height | single floor , double floors |
| Column | Q235 , Q345 welded H section steel |
| Beam | Q235 , Q345 welded H section steel |
| Purlin | Q235 C channel or Z channel |
| Knee brace | Q235 angle steel |
| Vertical and traversal support | Q235 angle steel , round bar or steel pipe |
| Tie bar | Q235 steel pipe |
| Brace | Q235 round bar |
| Cladding system | EPS , PU , Fiber glass wool sandwich panels or corrugated steel sheet with fiber glass wool insulation . *available in Different colors & gauge* |
| Partition wall | sandwich panels ( EPS , PU , Fiber glass wool etc . ) *available in Different colors & gauges* |
| Door | sandwich panel sliding door or roller door |
| Gutter | stainless steel or color steel sheet |
| Rainspout | PVC |
| Live load on roof | In 120kg / Sqm ( Color steel panel surrounded ) |
| Wind resistance grade | 12 grades |
| Earthquake-resistance | 8 - 9 grades |
| Structure usage | Up to 50 years |
| Finishing options | vast array of colors and textures available |
| Paint Options | Gray paint , red paint , white paint , epoxy zinc etc . Or Galvanized |