**components and materials of the JJJ ( made of CCC ) :**

|  |  |
| --- | --- |
| Main structure | Welded H section , Lattice structure , Tubular column or beam , space frame etc |
| Purlin | C Section Channel or Z Section Channel |
| Roof Cladding | Sandwich Panel or Corrugated Steel Sheet with Fiber Glass Wool Coil |
| Wall Cladding | Sandwich Panel or Corrugated Steel Sheet |
| Tie Rod | Circular Steel Tube |
| Brace | Round Bar |
| Column & Transverse Brace | Angle Steel or H Section Steel or Steel Pipe |
| Knee Brace | Angle Steel |
| Roof Gutter | Color Steel Sheet |
| Rainspout | PVC Pipe |
| Door | Sliding Sandwich Panel Door or Metal Door |
| Windows | PVC/Plastic Steel/Aluminum Alloy Window |
| Connecting | High Strength Bolts |
| Packing | Decided by you , loaded into 1X 40ft GP , 1X20 ft GP , 1X40 ft HQ |
| Drawing | We can make the design and quotation according to your require or your drawing |