### **Characteristics of JJJ ( made of CCC ) :**

Steel structure is widely used as warehouse , factory , hotel , church , garage etc . It is durable , economic and environmental .

****Main Grade :** Q345B , Q235B**

****Standard :** ISO9001 : 2008**

**We are a Factory-direct provider of all kinds of steel structure buildings and material plant . We specialize in design , fabricate construction , install and related technology guide . Our competitive price and high quality have got customers from all over the word .**

****Applications :****

**Used as Steel workshop / warehouse / shed , Exhibition Hall , Office buildings , Garage , Multi-story building , Hanger , Agricultural storage , Logistic centers , and all kinds of steel materials etc .**

****Specifications :****

**Main Steel : Q345B , Q235B**

**Column&Beam : Welded or Hot rolled H-section**

**Wall&Roof : EPS , Rock wall , PU sandwich , corrugated steel sheet**

**Door : Rolled up door or Sliding door**

**Window : Plastic steel or Aluminum alloy window**

**Surface : Hot dip galvanized or painted . ( all colors we can do )**

**Crane : 5T , 10T , 15T , etc .**